NOISE MONITORING LICENSE REQUIREMENTS

**L6 Noise limits**

L6.1 Noise from the brick manufacturing operations must not exceed an LA10 (15 minute) noise emission criterion of 50 dB(A), except as expressly provided by this licence.

L6.2 Noise from the premises is to be measured or computed at any point within six metres of any residence or other noise sensitive area in the vicinity of the premises to determine compliance with condition L6.1. 5dB(A) must be added if the noise is tonal or impulsive in character.